**Annex A**

**Specifications Table - Biloberizka ATC**

**Wheeled excavator-loader**

**Quantity: One (1)**

***Quantity subject to change upon availability of funds***

*Instructions: Please indicate in column B whether your quotation meets or does not meet the stated specification.*

|  |  |  |  |
| --- | --- | --- | --- |
|  | 1. **Technical Specifications** | | 1. **Bidder Response** |
| 1 | Excavator-loader JBC 3CX SITEMASTER or equivalent model must be brand new, manufactured in 2017 or later | |  |
| 2 | Excavator-loader on a pneumatic wheeled chassis, all wheels gear drive and hydraulic power steering. The machine must be a standard factory production. | |  |
| 3 | Four cylinder diesel engine, capacity not less than 4 l, power at least 67 kW/82 hp | |  |
| 4 | All four swivel wheels | |  |
| 5 | Load basket is multifunctional, width - not less than 220 sm | |  |
| 6 | The bucket must be adapted to fit the carriage | |  |
| 7 | The height of the unloading of the load bucket - not less than 2.7 m | |  |
| 8 | Load bucket bearing capacity on the maximum height – not less than 3200 kg | |  |
| 9 | The nominal capacity of the loader bucket is at least 1.0 cubic meters | |  |
| 10 | The excavator arm is telescopic | |  |
| 11 | Maximum digging depth of the excavator is not less than 4/5 m | |  |
| 12 | Bucket excavator width 60-80 sm, busket capacity – not less than 0.3 m | |  |
| 13 | Excavator bucket bearing capacity – up to 1450 kg | |  |
| 14 | Maximum height of unloading of excavator bucket – 3.8/4.7 m | |  |
| 15 | Turning angle of excavator bucket - not less than 200º | |  |
| 16 | Transmission: all wheels drive | |  |
| 17 | The loader arm must be equipped with an automatic hydraulic cushion system for front equipment/attachments during movement (smooth motion system) | |  |
| 18 | Additional excavator bucket width 400-450 mm | |  |
| 19 | Additional excavation grading bucket width 1500-1800 mm | |  |
| 20 | Quick replacement tool for excavator parts | |  |
| 21 | A carriage should be fitted for quick replacement of attachments on the loader’s arm | |  |
| 22 | Mandatory additional equipment: snow angle blade with amortization, turning angle +/- 300, width at least 2.5 m | |  |
| 23 | Reverse drive audible signal (option) | |  |
| 24 | Warranty: 12 months without limitation of working hours | |  |
| Requirements continues below | | | |
| **Other RFQ Requirements** | | | |
| 1 | **Annex B** | Completed, signed and submitted |  |
| 2 | **Ocean Shipment** | State whether or not a U.S. flag carrier is available |  |
| 3 | **Country of Manufacture** | Name the country of manufacture |  |
| 4 | **Source of Vehicles** | Name the country where vehicles are currently located |  |
| 5 | **Nationality of Bidder** | Name the country where bidder is registered for business |  |
| 6 | **After-Sales Service** | Name and location of authorized after-sales service in Ukraine |  |
| 7 | **Quotation validity** | No less than 60 days |  |
| 8 | **Warranty** | State the warranty terms |  |
| 9 | **Delivery** | State the number of calendar days for delivery |  |